Item No 05	Sheet 2-FCC-AC8 – Fancher Creek Elementary – MPR

a.	 Remove exterior door FCC-BMPR-DR05 from scope of work. Remove reference to reader, door hardware and associated cabling.

Item No 06	 Sheet 2-FCC-AC10 – Fancher Creek Elementary – MPR Photos a.	Removed photos of Door 05 at MPR.

Item No 07	Sheet 2-ORZ-AC2 – Oraze Elementary – Administration

a.          Modified routing of homerun cabling from door readers back to main access control panel to reduce the amount of surface mounted raceway needed for cabling installation.

Item No 08	Sheet 2-RIS-AC18 – Reyburn Intermediate - MPR

a.	Updated IDF layout for existing network rack location.

Item No 09	Sheet 2-RIS-AC20 – Reyburn Intermediate - MPR Photos

a.	Updated photos of existing telecom / electrical room in MPR Building

Item No 10	Sheet 2-TKE-AC8 – Temperance Kutner Elem - MPR

a.	Updated location of existing network rack and new access control panel. b.	Added keyed note to existing electrical panel at stage

End of Addendum 01

Page	of 2

CLOVIS USD CAMPUS SECURITY IMPROVEMENT PROJECT PHASE 2 SUMMARY OF WORK
PAGE 1

SUMMARY OF WORK – ADM 1

PART 1 - GENERAL

1.01 SUMMARY

A. General: Construction of BASE BID and Alternate portions of the work for Clovis Unified School District – Campus Security Improvement Project PHASE2 Fresno/Clovis, California. BASE BID and Alternate portionsof the workis defined as all material, labor, equipment and services necessary to do all work shown on the drawings and called for in the Specifications.

General Summary of the Project

The following information applies to all Bid packages and shall be reviewedcarefullyfor inclusion in each bid. Followingare critical logistics related to the Project:
1.Construction of new door lockdown system and improved PA system including all necessary new door hardware, card readers,cabling,powersupplies,new speakers,integrationintodistrictsystem,demoandpatchofanydisturbedfinishes. 2.All workfortheproject will beperformed duringthe hoursof7:00a.mto3:30p.m. Workwill be performedonanactive
campus with students and teachers present.

3.Submittals and material procurement shall begin immediately upon award or letter of intent from the District. 4.Material procurement is critical and shall be diligently pursued to meet the contract schedule.
5.Bid packages shall review the project completely prior to bidding the work.

6.Any substitution of details or materials must be pre-approved by the Architect, engineers and DSA. All substitution requests must be submitted per Notice To Contractors. Bid Packages are responsible for all costs and time delays required for substitution approval.

In addition to the summary ofwork for each Bid Package, the followingwill apply andbecome a part ofthe contract witheach respective Bid package.

Storm Water Pollution Prevention Plan and Dust Control 1.Not Applicable.

Alternates 1.None.

Submittals and material procurement

1.	Submittals and material procurement shall begin immediately upon award or letter of intent from the District. 2.	Material procurement is critical and shall be diligently pursued to meet the contract schedule.

Schedule

1.	Bid packages shall review the project and schedule completely prior to bidding the work.

2.	The bid package will be required to provide a schedule and crew sizing showing how the work will be accomplished within the given time frame.
3.	Per the Bid Schedule, Bid Packages will be on multiple sites simultaneously. Primes Contractors shall anticipate multiple crews to complete the work on time.

Crew Sizes

1.	All bidpackages shall review the scheduleandconfirmthattheycancrew the project accordinglypriortosubmittinga bid. Include with each bid minimum and maximum crew sizes projected for the project.

State Agency Requirements

1.	All work shall comply with OSHA requirements.

Coordination of work

CLOVIS USD CAMPUS SECURITY IMPROVEMENT PROJECT PHASE 2 SUMMARY OF WORK
PAGE 2

1.	Coordinationofworkduringthe preconstructionperiodisequallyas critical toresolvingall issues priortothe start of work. Bidpackage shall review the project,coordinate andquestionanyissues toallow resolutionpriortothe start of work.
2.	Review and verify all existing conditions.

3.	Provide all necessary temporary utilities for own work.

4.	All bidpackages shall attendcoordinationmeetingsandprovidecoordinationdrawingsforworkrelatedtoothertrades. Note conflicts and provide potential solutions to the architect for review. Coordination and drawing approval must occur prior to start of work. Bid packages shall attend a pre-installation meeting prior to thestart of their work onsite. All bidpackages shall be available forpre-installationmeetingsofotherbidpackagesforcoordinationofrelatedwork.
5.	Provide written request for information through the CM for layout information from related trades.

6.	Request and review all associated shop drawings for coordination and layout purposes prior to installation of related materials.
7.	Review all as-builts prior to starting work.

Site Logistics:

1.	Only company vehicles are allowed onsite. No tool drop-off or parking by personal vehicles will be allowed. Bid package to make provisions for transport or tool distribution needs.
2.	Lunch and breaks shall be at designated areas only. No other areas will be allowed.

3.	Storage areas will be confined to the areas designated by the CM. Staging areas around the building shall be coordinated with the CM. Storage onsite will be controlled due to limited space available.
4.	Daily cleanup and off haul is required for each trade for their own work debris.

General Items to be provided by each bid package:
1.	Protect all work, new and existing, from damage until acceptance by owner. 2.	Provide water and shade for own crews.
3.	Furnish all access to roof for own work if applicable.
4.	Furnishandinstall ownfloorprotection as needed(Tarps,plastic,plywood,etc neededtoprotect work forown scope) 5.	Furnish and install all physical layout for own work.
6.	Each bid package will be responsible for removal from the site of all debris generated by each bid package. Contractors are expected to provide vacuum clean up at work area each day.
7.	Secure all ladders and lifts each evening.
8.	Provide protection of all roofing when own work requires access on the roofing systems. 9.	Provide caution tape and/or barriers for open area work and traffic control.
10. Provide safe condition for own installations so as not to expose any person to a safety hazard per OSHA regulations. 11. Any substitution of details or materials must be pre approved by the Architect, Engineers and DSA. All substitution requestsmust be submittedtoMWCpriortobid. Thisbidpackage isresponsible forall costsandtimedelaysrequired
for substitution approval.
12. Review as-builts prior to starting work.
13. Provide copy of daily reports to Construction Manager each day work is performed on site.
14. Provide copy of weekly safety meeting sign in sheet to Construction Manager each week work is performed on site. 15. This project will be constructed on an active campus during school hours. Work will be performed around students and teachers. All employees working on site shall wear badges and pass CUSD background check. Any communication with teachers/students will not be acceptable and employees will be removed from the jobsite immediately. Any work that needs to be performed in/above classrooms will need to be completed before or after
school. Early morning after school shifts may be necessary to meet schedule requirements.

CLOVIS USD CAMPUS SECURITY IMPROVEMENT PROJECT PHASE 2 SUMMARY OF WORK
PAGE 3

CSI-01a– Door Hardware

Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections DIVISION 00 DIVISION 01
08 11 13	HOLLOW METAL DOORS AND FRAMES 08 71 00	DOOR HARDWARE
09 91 23	PAINTING

Refer to additional related specifications sections for work specifically included in this bid package noted below

General Items
1.	Furnish and install all layout for own work. 2.	Provide all power for own work.
3.	Provide full time supervision for own work/subcontractors while work is being performed on site at each campus location.
4.	Provide storagecontainerforconstructionmaterials/supplies. Materialwillnotbeallowedtobestoredinsidebuildings. 5.	See General Notes at beginning of summary of work specification section for other items.

Coordination with Other Trades –
1.	Coordinate physical connection to door hardware with low voltage contractor. 2.	Coordinate student access to allow proper student flow.

Furnish and Install Items
1.	Furnishandinstall all doorhardware. RefertoFOBitemsbelow foritemstobeinstalledbyelectricalpackage. Remove any existing door hardware required for installation of new hardware and turn over to District.
2.	Drill all necessary holes in doors and frames as required to allow for installation of own work. 3.	Provide X-Ray scanning and coring for any holes required in concrete/CMU walls/ceilings.
4.	Furnish and install new doors/frames where shown.
5.	Furnish and install key cores. Coordinate with District prior to start of work on each site.
6.	Furnish and install any cover plates as shown on drawings to cover any existing holes in doors/frames.
7.	Furnish and install any necessary patchwork/paint to damaged adjacent finishes as a result of installation of new door frames.
8.	Furnish and install paint at new doors/frames.
9.	Furnish and install temporary barrier at work locations to separate student/staff from work area (delineators, caution tape, etc.)
10. Furnish and install Velcro strap at panic hardware to “dog down” doors as needed during gap between installation of new door hardware and completion of low voltage equipment installation.
11. Include inbid$5000$20,000 allowancefortouchuppaint at existingdoorsreceivingnew hardware wherepaint touch up is required. This work will be performed on T&M. ADM 1

FOB Items
1.	Furnish FOB jobsite door hardware power supplies/battery backups to be installed by the Electrical/Low Voltage Contractor. ADM 1

Installation of FOB Items 1.	None

End of Bid Package

CLOVIS USD CAMPUS SECURITY IMPROVEMENT PROJECT PHASE 2 SUMMARY OF WORK
PAGE 4

CSI-02a – Electrical & Low Voltage

Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections DIVISION 00 DIVISION 01
06 10 00	ROUGH CARPENTRY

08 41 13	ALUMINUM FRAMED ENTRANCES AND STOREFRONTS 08 80 00	GLASS AND GLAZING
09 91 23	PAINTING

26 00 00	GENERAL ELECTRICAL

26 05 00	COMMON WORK RESULTS FOR ELECTRICAL 27 10 00	STRUCTURED CABLING SYSTEM
27 51 13	PAGING SYSTEMS
28 31 00	ACCESS CONTROL SYSTEM

Refer to additional related specifications sections for work specifically included in this bid package noted below

General Items
1.	Furnish and install all layout for own work 2.	Provide all power for own work.
3.	Provide full time supervision for own work/subcontractors while work is being performed on site.
4.	Provide storagecontainerforconstructionmaterials/supplies. Materialwillnotbeallowedtobestoredinsidebuildings. 5.	See General Notes at beginning of summary of work specification section for other items

Coordination with Other Trades
1.	Coordinate physical connection to door hardware with hardware contractor. 2.	Coordinate student access to allow proper student flow.
3.	Provide use ofelectrical equipment anddevices as requiredbythe ConstructionManagerfortestingofequipmentprior to final acceptance, which will not initiate the warranty period until filing of notice of completion.

Furnish and Install Items
1.	Furnish and install all required cabling for door lock and PA systems.
2.	Provide X-Ray scanning and coring for any holes required in concrete/CMU walls/ceilings.
3.	Furnish and install all surface mounted raceways for any cabling that can not be run inside walls/ceilings/frames. Wiring shall be routed through storefront/HM frames where possible. Grout filled frames shall receive surface mount wiremold. Emergency push button at front office desk shall be installed in wall adjacent to reception desk. Coordinate exact location with Owner prior to installation. Wiring to be concealed inside wall where possible.
4.	Furnish and install surface mount EMT conduit in gymnasiums. Paint conduit to match adjacent surroundings. 5.	Furnish and install ceiling wires and cable supports for cabling running above accessible ceiling. Brace every 4’. 6.	Remove and reinstall any glass in storefront/HM systems as required for access to own work.
7.	Remove andreinstall acoustical ceilingtilesas requiredforaccesstoownwork. Anydamagedtilesshallbereplacedat contractors expense.
8.	Furnish and install firestopping for own work as required at any penetrations through fire walls.
9.	Furnish andinstall all access doors necessary toprovideaccess to work included in this bidpackage. Provide required ceiling/soffit framing for installation of access doors. Paint access doors.
10. Furnish and install watertight closures at all penetrations through exterior walls.
11. Furnish and install all new speakers and cabling for PA system upgrade as shown on drawings. Make physical connection to existing system.
12. Drill all necessary holes/sleeves in walls, doors, and frames as required to allow for installation of own work. 13. Furnish and install all security/access control panels and power supplies for all buildings as required.
14. Make final connection/termination where cabling connects to door hardware.
15. Furnish and install power for door notifier/power supplies/battery back ups. Provide power from existing electrical panel to equipment location as called out on plans.

CLOVIS USD CAMPUS SECURITY IMPROVEMENT PROJECT PHASE 2 SUMMARY OF WORK
PAGE 5

16. Furnish and install emergency push button located at front desk as indicated on drawings.
17. Furnish and install lockable enclosure panel for all power supplies and battery back ups to allow for clean installation and to eliminate potential vandalism to equipment exposed to public view. Refer to drawings for exact locations and sizes.
18. Furnish and install network cabling to access control equipment.
19. Furnish and install card readers, security wiring, and headend equipment as specified. 20. Furnish and install interface relays, door position contacts, and request to exit devices.
21. Provide necessary patch/paint for damages (if any) to adjacent surroundings caused by installation of new materials installed under this contract.
22. Furnish and install temporary barrier at work locations to separate student/staff from work area (delineators, caution tape, etc.)

FOB Items 1.	None

Installation of FOB Items
1.	Install power supplies/battery back ups furnished FOB by Door Hardware Contractor. ADM 1
2.     Any equipment/material provided FOB from the door hardware bid package and installed by this bid package, the installing contractor shall meet all certifications/licensing requirements necessary to install and warranty the product.

End of Bid Package

CUSD District Wide Lockdown

n t

01
		OVERALL PHOTOS OF CLASSROOM BLDG 600 SECOND FLOOR

02 DOOR: CEH-B600-DR07	DOOR HARDWARE SET: #06	03 DOOR: CEH-B600-DR08	DOOR HARDWARE SET: #17

HW GROUP NO. 06	HW GROUP NO. 17

QTY	DESCRIPTION

1	EA	DOOR CORD

2	EA	99 LD COVER PLATE

1	EA	QEL CONVERSION KIT 1	EA	CARD READER
POWER SUPPLY

CATALOG NUMBER

798C-18 050589 040063
BY WORK OF DIVISION 28 BY WORK OF DIVISION 28
RE-USE BALANCE OF EXISTING HARDWARE

FINISH	MFR

626           SCE 628           VON
VON

QTY	DESCRIPTION

1	EA	ELECTRIC HINGE

1	EA	ELEC PANIC HARDWARE 1	EA	RIM CYLINDER
1	EA	FSIC CORE

1	EA	CARD READER

POWER SUPPLY

CATALOG NUMBER

5BB1HW 4.5 X 4.5 CON TW8 RX-QELX-PA-AX-99-NL-CON 20-057 ICX
23-030

BY WORK OF DIVISION 28 BY WORK OF DIVISION 28
RE-USE BALANCE OF EXISTING HARDWARE

FINISH	MFR

652	IVE 626	VON 626	SCH
626	SCH

CHANGE TO DOOR CORD WITH 626 FINISH DUE TO CONTINUOUS HINGE CONFIGURATION

1

DISTRICT-WIDE ACCESS CONTROL UPGRADES PACKAGE #2

MARK	DATE

03/18/24

ISSUE

ISSUE FOR PROPOSAL

ACCESS CONTROL - CLOVIS EAST HS PHOTOS - CLASSROOM 600 - FIRST FLOOR

2-CEH-AC16

Page 16 of 46

ACCESS CONTROL - GENERAL NOTES:

ALL LOW VOLTAGE CABLING IN EXPOSED AREAS SHALL BE INSTALLED IN SURFACE MOUNTED RACEWAY OR CONDUIT

ALL EXPOSED CONDUIT IN PUBLIC SPACES SHALL BE PAINTED TO MATCH EXISTING WALL OR CEILING COLOR

ALL ACCESS CONTROL WIRING SHALL BE GREEN IN COLOR

ALL LOW VOLTAGE WIRING NOT INSTALLED IN CONDUIT SHALL BE SUPPORTED EVERY 5' MINIMUM FROM APPROVED CABLING SUPPORT SYSTEM CONNECTED BACK TO BUILDING STRUCTURE

COORDINATE WITH OWNER TECHNOLOGY DEPARTMENT ON LABELING AND TERMINATION PUNCHDOWN OF NEW DATA CABLING ASSOCIATED WITH ACCESS CONTROL SYSTEM

CONTRACTOR TO REPAIR ANY HOLES IN EXISTING DOORS AND FRAMES AS A RESULT OF HARDWARE REPLACEMENT. CONTRACTOR TO REPAINT FRAMES AND DOORS TO MATCH EXISTING SURROUNDING COLOR FOR ANY AREAS EXPOSED WHERE OLD HARDWARE WAS REMOVED.

CONTRACTOR TO COORDINATE WITH OWNER ON ALL PROGRAMMING AND DOOR NUMBERING REQUIREMENTS ASSOCIATED WITH ACCESS CONTROL SYSTEM PRIOR TO ANY WORK TAKING PLACE

CONTRACTOR IS RESPONSIBLE FOR PROVIDING BUILDING MAPS FOR EACH CAMPUS BUILDING AND INTEGRATING WITH ACCESS CONTROL DOOR LOCATIONS TO INDICATE DOOR STATUS AND PROVIDE REMOTE OPERATION OF DOORS THRU ACCESS CONTROL SYSTEM

CONTRACTOR IS REQUIRED TO PROVIDE ALL DOOR HARDWARE, WIRING AND POWER SUPPLIES ASSOCIATED WITH THE INSTALLATION OF ACCESS CONTROL SYSTEM.

CONTRACTOR TO PROVIDE 120V. POWER, CONDUIT, WIRING AND BREAKERS ASSOCIATED WITH PROVIDING POWER TO ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES

CONTRACTOR SHALL COORDINATE WITH OWNER ON THE TRANSITION AND SCHEDULING OF ACCESS CONTROL SYSTEM ONCE ITS READY TO ACTIVATE FOR EACH BUILDING

CONTRACTOR SHALL MAINTAIN EXISTING WALL RATINGS FOR ANY PENETRATIONS THRU EXISTING RATED WALLS AS A RESULT OF ANY NEW CABLING BEING INSTALLED.

CONTRACTOR SHALL INSTALL A REQUEST TO EXIT "REX" DEVICE FOR ALL DOORS RECEIVING A CARD READER AND ELECTRIFIED HARDWARE INTERFACE. REX DEVICE SHALL PROVIDE STATUS OF BOTH DOORS. DEVICE TO BE WALL OR CEILING MOUNTED TO PROVIDE PROPER COVERAGE OF EXIT PATHWAY

ACCESS CONTROL - KEYED NOTES:

1	THIS DOOR SHALL RECEIVE A NEW CARD READER. CONTRACTOR SHALL REFER	5 TO DOOR HARDWARE SCHEDULE FOR WORK SCOPE REQUIRED. PROVIDE ALL

NEW HARDWARE, WIRING AND TERMINATIONS REQUIRED TO INSTALL NEW CARD READER AND ELECTRIFIED DOOR HARDWARE

2	LOCATION OF EXISTING MDF/IDF ROOM. ALL NEW ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES SHALL BE INSTALLED IN THIS ROOM.

3
LOCATION OF NEW ACCESS CONTROL PANEL AND DOOR POWER SUPPLIES	6 SHALL BE MOUNTED ON THE WALL AT THIS LOCATION. CONTRACTOR TO
INSTALL NEW CATEGORY 6 DATA CABLE FROM NEW ACCESS CONTROL PANEL BACK TO EXISTING PATCH PANEL IN EXISTING DATA RACK AND TERMINATE ON AVAILABLE PORT. CONTRACTOR TO INSTALL NEW WIRING IN SURFACE
MOUNTED RACEWAY OR ROUTED ON EXISTING LADDER RACK FROM ACCESS	7 CONTROL PANEL BACK TO RACK. CONTRACTOR TO INSTALL NEW 120V, 20A

DUPLEX RECEPTACLE IN ACCESS CONTROL PANEL AND CONNECT BACK TO EXISTING ELECTRICAL PANEL
4	FRONT ADMINISTRATION AREA TO RECEIVE NEW WALL MOUNTED LOCKDOWN	8 BUTTON WITH COVER IN THIS AREA. COORDINATE WITH OWNER ON FINAL
LOCATION OF BUTTON PRIOR TO INSTALLATION. CONTRACTOR TO PROVIDE LABELING OF BUTTON TO INDICATE "LOCKDOWN" ON COVER. BUTTON SHALL BE BLUE IN COLOR.

APPROXIMATE ROUTE OF MULTICONDUCTOR ACCESS CONTROL CABLE FROM	9 ACCESS CONTROL DOOR BACK TO HEADEND PANEL LOCATED IN MDF/IDF ROOM. CONTRACTOR SHALL BE RESPONSIBLE FOR ALL NEW RACEWAY OR ACCESS PANELS REQUIRED TO INSTALL ACCESS CONTROL WIRING ABOVE
INACCESSIBLE CEILINGS. ALL WIRING SHALL BE PROPERLY SUPPORTED FOR
FULL RUN. ANY WIRING PENETRATIONS PASSING THRU RATED WALL SHALL	10

MAINTAIN WALL RATING AFTER WIRING IS INSTALLED.

LOCATION OF EXISTING 120V ELECTRICAL PANEL. CONTRACTOR TO ROUTE NEW 120V, 20A BRANCH CIRCUIT FROM NEW ACCESS CONTROL PANEL BACK TO
THIS LOCATION. CONTRACTOR SHALL INSTALL NEW 120V, 20A BREAKER IN	11 AVAILABLE SPACE IN THIS PANEL.

LOCATION OF EXISTING FLOOR MOUNTED NETWORK RACKS. ALL NEW DATA CABLING SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON EXISTING PATCH PANEL.

LOCATION OF EXISTING INTERCOM WALL MOUNTED PUNCHDOWN BLOCK. ALL NEW SPEAKERS SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON TERMINAL STRIP. CONTRACTOR TO CONFIGURE EXISTING INTERCOM SYSTEM TO ADD ANY NEW EXTERIOR SPEAKER AND ZONES TO EXISTING SYSTEM AS REQUIRED.

CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE,
NON-POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION.

THIS AREA HAS AN OPEN CEILING AREA OR INACCESSIBLE CEILING AREA, CONDUIT WILL BE REQUIRED TO ROUTE THRU OPEN AREAS OR ACCESS PANELS NEEDED TO ACCESS ABOVE INACCESSIBLE CEILINGS TO ALLOW CABLING TO BE INSTALLED.

CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE, POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION. PROVIDE LOCAL POWER TRANSFORMER AND TERMINATIONS REQUIRED TO POWER SPEAKER

CR

REX

1	RE:2-CEH-AC36

		
CR

REX

CR
CR

REX	REX

CEH-BGW-DR01

1

RE:2-CEH-AC36

CEH-BGW-DR02

1	RE:2-CEH-AC37	5 CEH-BGW-DR03

1	RE:2-CEH-AC37 CEH-BGW-DR04

6	3

7

2 1

CR

8

REX

1	RE:2-CEH-AC39 CEH-BGW-DR09

5

1

								

10

10

						

						

								

RE:2-CEH-AC38

CEH-BGW-DR07

1	RE:2-CEH-AC38 CEH-BGW-DR08

REX

1	RE:2-CEH-AC38

CEH-BGW-DR06	5

REX	REX

1	RE:2-CEH-AC37

CEH-BGW-DR05 REX

CR	CR	CR
CR
CLOVIS EAST HS - GYMNASIUM - WEST

SCALE: 1/16"=1'-0"

DISTRICT-WIDE ACCESS CONTROL UPGRADES PACKAGE #2

MARK	DATE

03/18/24

ISSUE

ISSUE FOR PROPOSAL

ACCESS CONTROL - CLOVIS EAST HS GYMNASIUM - WEST

2-CEH-AC35

Page 35 of 46

8	3

6	7

1

2

ACCESS CONTROL - GENERAL NOTES:

ALL LOW VOLTAGE CABLING IN EXPOSED AREAS SHALL BE INSTALLED IN SURFACE MOUNTED RACEWAY OR CONDUIT

ALL EXPOSED CONDUIT IN PUBLIC SPACES SHALL BE PAINTED TO MATCH EXISTING WALL OR CEILING COLOR

ALL ACCESS CONTROL WIRING SHALL BE GREEN IN COLOR

ALL LOW VOLTAGE WIRING NOT INSTALLED IN CONDUIT SHALL BE SUPPORTED EVERY 5' MINIMUM FROM APPROVED CABLING SUPPORT SYSTEM CONNECTED BACK TO BUILDING STRUCTURE

COORDINATE WITH OWNER TECHNOLOGY DEPARTMENT ON LABELING AND TERMINATION PUNCHDOWN OF NEW DATA CABLING ASSOCIATED WITH ACCESS CONTROL SYSTEM

CONTRACTOR TO REPAIR ANY HOLES IN EXISTING DOORS AND FRAMES AS A RESULT OF HARDWARE REPLACEMENT. CONTRACTOR TO REPAINT FRAMES AND DOORS TO MATCH EXISTING SURROUNDING COLOR FOR ANY AREAS EXPOSED WHERE OLD HARDWARE WAS REMOVED.

CONTRACTOR TO COORDINATE WITH OWNER ON ALL PROGRAMMING AND DOOR NUMBERING REQUIREMENTS ASSOCIATED WITH ACCESS CONTROL SYSTEM PRIOR TO ANY WORK TAKING PLACE

CONTRACTOR IS RESPONSIBLE FOR PROVIDING BUILDING MAPS FOR EACH CAMPUS BUILDING AND INTEGRATING WITH ACCESS CONTROL DOOR LOCATIONS TO INDICATE DOOR STATUS AND PROVIDE REMOTE OPERATION OF DOORS THRU ACCESS CONTROL SYSTEM

CONTRACTOR IS REQUIRED TO PROVIDE ALL DOOR HARDWARE, WIRING AND POWER SUPPLIES ASSOCIATED WITH THE INSTALLATION OF ACCESS CONTROL SYSTEM.

CONTRACTOR TO PROVIDE 120V. POWER, CONDUIT, WIRING AND BREAKERS ASSOCIATED WITH PROVIDING POWER TO ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES

CONTRACTOR SHALL COORDINATE WITH OWNER ON THE TRANSITION AND SCHEDULING OF ACCESS CONTROL SYSTEM ONCE ITS READY TO ACTIVATE FOR EACH BUILDING

CONTRACTOR SHALL MAINTAIN EXISTING WALL RATINGS FOR ANY PENETRATIONS THRU EXISTING RATED WALLS AS A RESULT OF ANY NEW CABLING BEING INSTALLED.

CONTRACTOR SHALL INSTALL A REQUEST TO EXIT "REX" DEVICE FOR ALL DOORS RECEIVING A CARD READER AND ELECTRIFIED HARDWARE INTERFACE. REX DEVICE SHALL PROVIDE STATUS OF BOTH DOORS. DEVICE TO BE WALL OR CEILING MOUNTED TO PROVIDE PROPER COVERAGE OF EXIT PATHWAY

ACCESS CONTROL - KEYED NOTES:

REX

LIBRARY BUILDING - FANCHER CREEK ELEMENTARY SCALE: 1/16"=1'-0"

1	RE:2-FCC-AC6 FCC-BL-DR01

1

2

3

4

5

6

7

8

9

10

11

THIS DOOR SHALL RECEIVE A NEW CARD READER. CONTRACTOR SHALL REFER TO DOOR HARDWARE SCHEDULE FOR WORK SCOPE REQUIRED. PROVIDE ALL NEW HARDWARE, WIRING AND TERMINATIONS REQUIRED TO INSTALL NEW CARD READER AND ELECTRIFIED DOOR HARDWARE

LOCATION OF EXISTING MDF/IDF ROOM. ALL NEW ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES SHALL BE INSTALLED IN THIS ROOM.

LOCATION OF NEW ACCESS CONTROL PANEL AND DOOR POWER SUPPLIES SHALL BE MOUNTED ON THE WALL AT THIS LOCATION. CONTRACTOR TO INSTALL NEW CATEGORY 6 DATA CABLE FROM NEW ACCESS CONTROL PANEL BACK TO EXISTING PATCH PANEL IN EXISTING DATA RACK AND TERMINATE ON AVAILABLE PORT. CONTRACTOR TO INSTALL NEW WIRING IN SURFACE MOUNTED RACEWAY OR ROUTED ON EXISTING LADDER RACK FROM ACCESS CONTROL PANEL BACK TO RACK. CONTRACTOR TO INSTALL NEW 120V, 20A DUPLEX RECEPTACLE IN ACCESS CONTROL PANEL AND CONNECT BACK TO EXISTING ELECTRICAL PANEL

FRONT ADMINISTRATION AREA TO RECEIVE NEW WALL MOUNTED LOCKDOWN BUTTON WITH COVER IN THIS AREA. COORDINATE WITH OWNER ON FINAL LOCATION OF BUTTON PRIOR TO INSTALLATION. CONTRACTOR TO PROVIDE LABELING OF BUTTON TO INDICATE "LOCKDOWN" ON COVER. BUTTON SHALL BE BLUE IN COLOR.

APPROXIMATE ROUTE OF MULTICONDUCTOR ACCESS CONTROL CABLE FROM ACCESS CONTROL DOOR BACK TO HEADEND PANEL LOCATED IN MDF/IDF ROOM. CONTRACTOR SHALL BE RESPONSIBLE FOR ALL NEW RACEWAY OR ACCESS PANELS REQUIRED TO INSTALL ACCESS CONTROL WIRING ABOVE INACCESSIBLE CEILINGS. ALL WIRING SHALL BE PROPERLY SUPPORTED FOR FULL RUN. ANY WIRING PENETRATIONS PASSING THRU RATED WALL SHALL MAINTAIN WALL RATING AFTER WIRING IS INSTALLED.

LOCATION OF EXISTING 120V ELECTRICAL PANEL. CONTRACTOR TO ROUTE NEW 120V, 20A BRANCH CIRCUIT FROM NEW ACCESS CONTROL PANEL BACK TO THIS LOCATION. CONTRACTOR SHALL INSTALL NEW 120V, 20A BREAKER IN AVAILABLE SPACE IN THIS PANEL.

LOCATION OF EXISTING FLOOR MOUNTED NETWORK RACKS. ALL NEW DATA CABLING SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON EXISTING PATCH PANEL.

LOCATION OF EXISTING INTERCOM WALL MOUNTED PUNCHDOWN BLOCK. ALL NEW SPEAKERS SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON TERMINAL STRIP. CONTRACTOR TO CONFIGURE EXISTING INTERCOM SYSTEM TO ADD ANY NEW EXTERIOR SPEAKER AND ZONES TO EXISTING SYSTEM AS REQUIRED.

CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE,
NON-POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION.

THIS AREA HAS AN OPEN CEILING AREA OR INACCESSIBLE CEILING AREA, CONDUIT WILL BE REQUIRED TO ROUTE THRU OPEN AREAS OR ACCESS PANELS NEEDED TO ACCESS ABOVE INACCESSIBLE CEILINGS TO ALLOW CABLING TO BE INSTALLED.

CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE, POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION. PROVIDE LOCAL POWER TRANSFORMER AND TERMINATIONS REQUIRED TO POWER SPEAKER

DISTRICT-WIDE ACCESS CONTROL UPGRADES PACKAGE #2

MARK	DATE

03/18/24

ISSUE

ISSUE FOR PROPOSAL

ACCESS CONTROL - FANCHER CREEK ES LIBRARY BUILDING PLAN

2-FCC-AC5

Page 5 of 10

01 OVERALL PHOTOS OF LIBRARY AREAS	02 DOOR: FCC-BL-DR01	DOOR HARDWARE SET: #23

HW GROUP NO. 23

QTY	DESCRIPTION

1	EA	STOREROOM LOCK 1	EA	MORTISE CYLINDER 1	EA	ELECTRIC STRIKE
1	EA	CARD READER

POWER SUPPLY

CATALOG NUMBER

L9080L 06L

RE-USE EXISTING

6400 FSE 12/24 VAC/VDC BY WORK OF DIVISION 28 BY WORK OF DIVISION 28
RE-USE BALANCE OF EXISTING HARDWARE

FINISH	MFR

626           SCH 626           SCH
630	VON

1

DISTRICT-WIDE ACCESS CONTROL UPGRADES PACKAGE #2

MARK	DATE

03/18/24

ISSUE

ISSUE FOR PROPOSAL

ACCESS CONTROL - FANCHER CREEK ES PHOTOS - LIBRARY BLDG

2-FCC-AC6

Page 6 of 10

7	2

ACCESS CONTROL - GENERAL NOTES:

ALL LOW VOLTAGE CABLING IN EXPOSED AREAS SHALL BE INSTALLED IN SURFACE MOUNTED RACEWAY OR CONDUIT

ALL EXPOSED CONDUIT IN PUBLIC SPACES SHALL BE PAINTED TO MATCH EXISTING WALL OR CEILING COLOR

ALL ACCESS CONTROL WIRING SHALL BE GREEN IN COLOR

ALL LOW VOLTAGE WIRING NOT INSTALLED IN CONDUIT SHALL BE SUPPORTED EVERY 5' MINIMUM FROM APPROVED CABLING SUPPORT SYSTEM CONNECTED BACK TO BUILDING STRUCTURE

COORDINATE WITH OWNER TECHNOLOGY DEPARTMENT ON LABELING AND TERMINATION PUNCHDOWN OF NEW DATA CABLING ASSOCIATED WITH ACCESS CONTROL SYSTEM

3 5

5

1	10	5

6

CONTRACTOR TO REPAIR ANY HOLES IN EXISTING DOORS AND FRAMES AS A RESULT OF HARDWARE REPLACEMENT. CONTRACTOR TO REPAINT FRAMES AND DOORS TO MATCH EXISTING SURROUNDING COLOR FOR ANY AREAS EXPOSED WHERE OLD HARDWARE WAS REMOVED.

CONTRACTOR TO COORDINATE WITH OWNER ON ALL PROGRAMMING AND DOOR NUMBERING REQUIREMENTS ASSOCIATED WITH ACCESS CONTROL SYSTEM PRIOR TO ANY WORK TAKING PLACE

CONTRACTOR IS RESPONSIBLE FOR PROVIDING BUILDING MAPS FOR EACH CAMPUS BUILDING AND INTEGRATING WITH ACCESS CONTROL DOOR LOCATIONS TO INDICATE DOOR STATUS AND PROVIDE REMOTE OPERATION OF DOORS THRU ACCESS CONTROL SYSTEM

CONTRACTOR IS REQUIRED TO PROVIDE ALL DOOR HARDWARE, WIRING AND POWER SUPPLIES ASSOCIATED WITH THE INSTALLATION OF ACCESS CONTROL SYSTEM.

CONTRACTOR TO PROVIDE 120V. POWER, CONDUIT, WIRING AND BREAKERS ASSOCIATED WITH PROVIDING POWER TO ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES

CONTRACTOR SHALL COORDINATE WITH OWNER ON THE TRANSITION AND SCHEDULING OF ACCESS CONTROL SYSTEM ONCE ITS READY TO ACTIVATE FOR EACH BUILDING

CONTRACTOR SHALL MAINTAIN EXISTING WALL RATINGS FOR ANY PENETRATIONS THRU EXISTING RATED WALLS AS A RESULT OF ANY NEW CABLING BEING INSTALLED.

CONTRACTOR SHALL INSTALL A REQUEST TO EXIT "REX" DEVICE FOR ALL DOORS RECEIVING A CARD READER AND ELECTRIFIED HARDWARE INTERFACE. REX DEVICE SHALL PROVIDE STATUS OF BOTH DOORS. DEVICE TO BE WALL OR CEILING MOUNTED TO PROVIDE PROPER COVERAGE OF EXIT PATHWAY

ACCESS CONTROL - KEYED NOTES:

1

		CR

REX	2

THIS DOOR SHALL RECEIVE A NEW CARD READER. CONTRACTOR SHALL REFER TO DOOR HARDWARE SCHEDULE FOR WORK SCOPE REQUIRED. PROVIDE ALL NEW HARDWARE, WIRING AND TERMINATIONS REQUIRED TO INSTALL NEW CARD READER AND ELECTRIFIED DOOR HARDWARE

LOCATION OF EXISTING MDF/IDF ROOM. ALL NEW ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES SHALL BE INSTALLED IN THIS ROOM.

1	3 REX	RE:2-FCC-AC9
5	CR	FCC-BMPR-DR04

RE:2-FCC-AC9	4 1	FCC-BMPR-DR03

5

6

REX	REX

LOCATION OF NEW ACCESS CONTROL PANEL AND DOOR POWER SUPPLIES SHALL BE MOUNTED ON THE WALL AT THIS LOCATION. CONTRACTOR TO INSTALL NEW CATEGORY 6 DATA CABLE FROM NEW ACCESS CONTROL PANEL BACK TO EXISTING PATCH PANEL IN EXISTING DATA RACK AND TERMINATE ON AVAILABLE PORT. CONTRACTOR TO INSTALL NEW WIRING IN SURFACE MOUNTED RACEWAY OR ROUTED ON EXISTING LADDER RACK FROM ACCESS CONTROL PANEL BACK TO RACK. CONTRACTOR TO INSTALL NEW 120V, 20A DUPLEX RECEPTACLE IN ACCESS CONTROL PANEL AND CONNECT BACK TO EXISTING ELECTRICAL PANEL

FRONT ADMINISTRATION AREA TO RECEIVE NEW WALL MOUNTED LOCKDOWN BUTTON WITH COVER IN THIS AREA. COORDINATE WITH OWNER ON FINAL LOCATION OF BUTTON PRIOR TO INSTALLATION. CONTRACTOR TO PROVIDE LABELING OF BUTTON TO INDICATE "LOCKDOWN" ON COVER. BUTTON SHALL BE BLUE IN COLOR.

APPROXIMATE ROUTE OF MULTICONDUCTOR ACCESS CONTROL CABLE FROM ACCESS CONTROL DOOR BACK TO HEADEND PANEL LOCATED IN MDF/IDF ROOM. CONTRACTOR SHALL BE RESPONSIBLE FOR ALL NEW RACEWAY OR ACCESS PANELS REQUIRED TO INSTALL ACCESS CONTROL WIRING ABOVE INACCESSIBLE CEILINGS. ALL WIRING SHALL BE PROPERLY SUPPORTED FOR FULL RUN. ANY WIRING PENETRATIONS PASSING THRU RATED WALL SHALL MAINTAIN WALL RATING AFTER WIRING IS INSTALLED.

LOCATION OF EXISTING 120V ELECTRICAL PANEL. CONTRACTOR TO ROUTE NEW 120V, 20A BRANCH CIRCUIT FROM NEW ACCESS CONTROL PANEL BACK TO THIS LOCATION. CONTRACTOR SHALL INSTALL NEW 120V, 20A BREAKER IN AVAILABLE SPACE IN THIS PANEL.

CR

RE:2-FCC-AC9

CR

RE:2-FCC-AC9

1	FCC-BMPR-DR02

7	LOCATION OF EXISTING FLOOR MOUNTED NETWORK RACKS. ALL NEW DATA CABLING SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON

EXISTING PATCH PANEL.

8	LOCATION OF EXISTING INTERCOM WALL MOUNTED PUNCHDOWN BLOCK. ALL NEW SPEAKERS SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON TERMINAL STRIP. CONTRACTOR TO CONFIGURE EXISTING INTERCOM SYSTEM TO ADD ANY NEW EXTERIOR SPEAKER AND ZONES TO EXISTING SYSTEM AS REQUIRED.

9	CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE,
NON-POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION.

1	FCC-BMPR-DR01

MULTI-PURPOSE BUILDING - FANCHER CREEK ELEMENTARY SCALE: 1/16"=1'-0"

10         THIS AREA HAS AN OPEN CEILING AREA OR INACCESSIBLE CEILING AREA, CONDUIT WILL BE REQUIRED TO ROUTE THRU OPEN AREAS OR ACCESS PANELS NEEDED TO ACCESS ABOVE INACCESSIBLE CEILINGS TO ALLOW CABLING TO BE INSTALLED.

11         CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE, POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION. PROVIDE LOCAL POWER TRANSFORMER AND TERMINATIONS REQUIRED TO POWER SPEAKER

DISTRICT-WIDE ACCESS CONTROL UPGRADES PACKAGE #2

MARK	DATE

03/18/24

ISSUE

ISSUE FOR PROPOSAL

ACCESS CONTROL - FANCHER CREEK ES MULTI-PURPOSE BUILDING PLAN

2-FCC-AC8

Page 8 of 10

LOCATION OF NEW ACCESS CONTROL PANEL

02 ELECTRICAL PANEL NEAR FRONT OF STAGE AREA	03 IDF AT MULTIPURPOSE MAINTENANCE AREA ADDITIONAL DOOR HARDWARE NOTES:

1. X

1

DISTRICT-WIDE ACCESS CONTROL UPGRADES PACKAGE #2

MARK	DATE

03/18/24

ISSUE

ISSUE FOR PROPOSAL

ACCESS CONTROL - FANCHER CREEK ES PHOTOS - MULTI-PURPOSE BLDG

2-FCC-AC10

Page 10 of 10

10	1	RE:2-ORZ-AC3 ORZ-BL-DR01

ACCESS CONTROL - GENERAL NOTES:

ALL LOW VOLTAGE CABLING IN EXPOSED AREAS SHALL BE INSTALLED IN SURFACE MOUNTED RACEWAY OR CONDUIT

ALL EXPOSED CONDUIT IN PUBLIC SPACES SHALL BE PAINTED TO MATCH EXISTING WALL OR CEILING COLOR

ALL ACCESS CONTROL WIRING SHALL BE GREEN IN COLOR

ALL LOW VOLTAGE WIRING NOT INSTALLED IN CONDUIT SHALL BE SUPPORTED EVERY 5' MINIMUM FROM APPROVED CABLING SUPPORT SYSTEM CONNECTED BACK TO BUILDING STRUCTURE

COORDINATE WITH OWNER TECHNOLOGY DEPARTMENT ON LABELING AND TERMINATION PUNCHDOWN OF NEW DATA CABLING ASSOCIATED WITH ACCESS CONTROL SYSTEM

CONTRACTOR TO REPAIR ANY HOLES IN EXISTING DOORS AND FRAMES AS A RESULT OF HARDWARE REPLACEMENT. CONTRACTOR TO REPAINT FRAMES AND DOORS TO MATCH EXISTING SURROUNDING COLOR FOR ANY AREAS EXPOSED WHERE OLD HARDWARE WAS REMOVED.

CONTRACTOR TO COORDINATE WITH OWNER ON ALL PROGRAMMING AND DOOR NUMBERING REQUIREMENTS ASSOCIATED WITH ACCESS CONTROL SYSTEM PRIOR TO ANY WORK TAKING PLACE

CONTRACTOR IS RESPONSIBLE FOR PROVIDING BUILDING MAPS FOR EACH CAMPUS BUILDING AND INTEGRATING WITH ACCESS CONTROL DOOR LOCATIONS TO INDICATE DOOR STATUS AND PROVIDE REMOTE OPERATION OF DOORS THRU ACCESS CONTROL SYSTEM

CONTRACTOR IS REQUIRED TO PROVIDE ALL DOOR HARDWARE, WIRING AND POWER SUPPLIES ASSOCIATED WITH THE INSTALLATION OF ACCESS CONTROL SYSTEM.

CONTRACTOR TO PROVIDE 120V. POWER, CONDUIT, WIRING AND BREAKERS ASSOCIATED WITH PROVIDING POWER TO ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES

CONTRACTOR SHALL COORDINATE WITH OWNER ON THE TRANSITION AND SCHEDULING OF ACCESS CONTROL SYSTEM ONCE ITS READY TO ACTIVATE FOR EACH BUILDING

CONTRACTOR SHALL MAINTAIN EXISTING WALL RATINGS FOR ANY PENETRATIONS THRU EXISTING RATED WALLS AS A RESULT OF ANY NEW CABLING BEING INSTALLED.

CONTRACTOR SHALL INSTALL A REQUEST TO EXIT "REX" DEVICE FOR ALL DOORS RECEIVING A CARD READER AND ELECTRIFIED HARDWARE INTERFACE. REX DEVICE SHALL PROVIDE STATUS OF BOTH DOORS. DEVICE TO BE WALL OR CEILING MOUNTED TO PROVIDE PROPER COVERAGE OF EXIT PATHWAY

ACCESS CONTROL - KEYED NOTES:

1

5	2

3	7	3

8	2	4

10	1	RE:2-ORZ-AC3	4 6                                                                                                           ORZ-BA-DR01

5 5

1

6

7

8

9

THIS DOOR SHALL RECEIVE A NEW CARD READER. CONTRACTOR SHALL REFER TO DOOR HARDWARE SCHEDULE FOR WORK SCOPE REQUIRED. PROVIDE ALL NEW HARDWARE, WIRING AND TERMINATIONS REQUIRED TO INSTALL NEW CARD READER AND ELECTRIFIED DOOR HARDWARE

LOCATION OF EXISTING MDF/IDF ROOM. ALL NEW ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES SHALL BE INSTALLED IN THIS ROOM.

LOCATION OF NEW ACCESS CONTROL PANEL AND DOOR POWER SUPPLIES SHALL BE MOUNTED ON THE WALL AT THIS LOCATION. CONTRACTOR TO INSTALL NEW CATEGORY 6 DATA CABLE FROM NEW ACCESS CONTROL PANEL BACK TO EXISTING PATCH PANEL IN EXISTING DATA RACK AND TERMINATE ON AVAILABLE PORT. CONTRACTOR TO INSTALL NEW WIRING IN SURFACE MOUNTED RACEWAY OR ROUTED ON EXISTING LADDER RACK FROM ACCESS CONTROL PANEL BACK TO RACK. CONTRACTOR TO INSTALL NEW 120V, 20A DUPLEX RECEPTACLE IN ACCESS CONTROL PANEL AND CONNECT BACK TO EXISTING ELECTRICAL PANEL

FRONT ADMINISTRATION AREA TO RECEIVE NEW WALL MOUNTED LOCKDOWN BUTTON WITH COVER IN THIS AREA. COORDINATE WITH OWNER ON FINAL LOCATION OF BUTTON PRIOR TO INSTALLATION. CONTRACTOR TO PROVIDE LABELING OF BUTTON TO INDICATE "LOCKDOWN" ON COVER. BUTTON SHALL BE BLUE IN COLOR.

APPROXIMATE ROUTE OF MULTICONDUCTOR ACCESS CONTROL CABLE FROM ACCESS CONTROL DOOR BACK TO HEADEND PANEL LOCATED IN MDF/IDF ROOM. CONTRACTOR SHALL BE RESPONSIBLE FOR ALL NEW RACEWAY OR ACCESS PANELS REQUIRED TO INSTALL ACCESS CONTROL WIRING ABOVE INACCESSIBLE CEILINGS. ALL WIRING SHALL BE PROPERLY SUPPORTED FOR FULL RUN. ANY WIRING PENETRATIONS PASSING THRU RATED WALL SHALL MAINTAIN WALL RATING AFTER WIRING IS INSTALLED.

LOCATION OF EXISTING 120V ELECTRICAL PANEL. CONTRACTOR TO ROUTE NEW 120V, 20A BRANCH CIRCUIT FROM NEW ACCESS CONTROL PANEL BACK TO THIS LOCATION. CONTRACTOR SHALL INSTALL NEW 120V, 20A BREAKER IN AVAILABLE SPACE IN THIS PANEL.

LOCATION OF EXISTING FLOOR MOUNTED NETWORK RACKS. ALL NEW DATA CABLING SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON EXISTING PATCH PANEL.

LOCATION OF EXISTING INTERCOM WALL MOUNTED PUNCHDOWN BLOCK. ALL NEW SPEAKERS SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON TERMINAL STRIP. CONTRACTOR TO CONFIGURE EXISTING INTERCOM SYSTEM TO ADD ANY NEW EXTERIOR SPEAKER AND ZONES TO EXISTING SYSTEM AS REQUIRED.

CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE,
NON-POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION.

ADMINISTRATION BUILDING - ORAZE ELEMENTARY SCALE: 1/16"=1'-0"

10         THIS AREA HAS AN OPEN CEILING AREA OR INACCESSIBLE CEILING AREA, CONDUIT WILL BE REQUIRED TO ROUTE THRU OPEN AREAS OR ACCESS PANELS NEEDED TO ACCESS ABOVE INACCESSIBLE CEILINGS TO ALLOW CABLING TO BE INSTALLED.

11         CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE, POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION. PROVIDE LOCAL POWER TRANSFORMER AND TERMINATIONS REQUIRED TO POWER SPEAKER

DISTRICT-WIDE ACCESS CONTROL UPGRADES PACKAGE #2

MARK	DATE

03/18/24

ISSUE

ISSUE FOR PROPOSAL

ACCESS CONTROL - ORAZE ELEMENTARY ADMINISTRATION BUILDING PLAN

2-ORZ-AC2

	
REX

		
RE
	X

CR

Page 2 of 17

ACCESS CONTROL - GENERAL NOTES:

ALL LOW VOLTAGE CABLING IN EXPOSED AREAS SHALL BE INSTALLED IN SURFACE MOUNTED RACEWAY OR CONDUIT

ALL EXPOSED CONDUIT IN PUBLIC SPACES SHALL BE PAINTED TO MATCH EXISTING WALL OR CEILING COLOR

ALL ACCESS CONTROL WIRING SHALL BE GREEN IN COLOR

ALL LOW VOLTAGE WIRING NOT INSTALLED IN CONDUIT SHALL BE SUPPORTED EVERY 5' MINIMUM FROM APPROVED CABLING SUPPORT SYSTEM CONNECTED BACK TO BUILDING STRUCTURE

COORDINATE WITH OWNER TECHNOLOGY DEPARTMENT ON LABELING AND TERMINATION PUNCHDOWN OF NEW DATA CABLING ASSOCIATED WITH ACCESS CONTROL SYSTEM

CONTRACTOR TO REPAIR ANY HOLES IN EXISTING DOORS AND FRAMES AS A RESULT OF HARDWARE REPLACEMENT. CONTRACTOR TO REPAINT FRAMES AND DOORS TO MATCH EXISTING SURROUNDING COLOR FOR ANY AREAS EXPOSED WHERE OLD HARDWARE WAS REMOVED.

CONTRACTOR TO COORDINATE WITH OWNER ON ALL PROGRAMMING AND DOOR NUMBERING REQUIREMENTS ASSOCIATED WITH ACCESS CONTROL SYSTEM PRIOR TO ANY WORK TAKING PLACE

CONTRACTOR IS RESPONSIBLE FOR PROVIDING BUILDING MAPS FOR EACH CAMPUS BUILDING AND INTEGRATING WITH ACCESS CONTROL DOOR LOCATIONS TO INDICATE DOOR STATUS AND PROVIDE REMOTE OPERATION OF DOORS THRU ACCESS CONTROL SYSTEM

CONTRACTOR IS REQUIRED TO PROVIDE ALL DOOR HARDWARE, WIRING AND POWER SUPPLIES ASSOCIATED WITH THE INSTALLATION OF ACCESS CONTROL SYSTEM.

CONTRACTOR TO PROVIDE 120V. POWER, CONDUIT, WIRING AND BREAKERS ASSOCIATED WITH PROVIDING POWER TO ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES

CONTRACTOR SHALL COORDINATE WITH OWNER ON THE TRANSITION AND SCHEDULING OF ACCESS CONTROL SYSTEM ONCE ITS READY TO ACTIVATE FOR EACH BUILDING

CONTRACTOR SHALL MAINTAIN EXISTING WALL RATINGS FOR ANY PENETRATIONS THRU EXISTING RATED WALLS AS A RESULT OF ANY NEW CABLING BEING INSTALLED.

CONTRACTOR SHALL INSTALL A REQUEST TO EXIT "REX" DEVICE FOR ALL DOORS RECEIVING A CARD READER AND ELECTRIFIED HARDWARE INTERFACE. REX DEVICE SHALL PROVIDE STATUS OF BOTH DOORS. DEVICE TO BE WALL OR CEILING MOUNTED TO PROVIDE PROPER COVERAGE OF EXIT PATHWAY

												

																			

																					

																		

									
						
REX

5 1	RE:2-RIS-AC20
RIS-BMPR-DR04

1	RE:2-RIS-AC20 RIS-BMPR-DR03

		REX

					
	CR

		

5

REX	REX

CR	CR

1	RE:2-RIS-AC19 RIS-BMPR-DR02

1	RE:2-RIS-AC19 RIS-BMPR-DR01

8	7

6

2

3

HIGH ON WALL

1

ACCESS CONTROL - KEYED NOTES:

1	THIS DOOR SHALL RECEIVE A NEW CARD READER. CONTRACTOR SHALL REFER TO DOOR HARDWARE SCHEDULE FOR WORK SCOPE REQUIRED. PROVIDE ALL

NEW HARDWARE, WIRING AND TERMINATIONS REQUIRED TO INSTALL NEW CARD READER AND ELECTRIFIED DOOR HARDWARE

2	LOCATION OF EXISTING MDF/IDF ROOM. ALL NEW ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES SHALL BE INSTALLED IN THIS ROOM.

3
LOCATION OF NEW ACCESS CONTROL PANEL AND DOOR POWER SUPPLIES SHALL BE MOUNTED ON THE WALL AT THIS LOCATION. CONTRACTOR TO INSTALL NEW CATEGORY 6 DATA CABLE FROM NEW ACCESS CONTROL PANEL BACK TO EXISTING PATCH PANEL IN EXISTING DATA RACK AND TERMINATE ON AVAILABLE PORT. CONTRACTOR TO INSTALL NEW WIRING IN SURFACE MOUNTED RACEWAY OR ROUTED ON EXISTING LADDER RACK FROM ACCESS CONTROL PANEL BACK TO RACK. CONTRACTOR TO INSTALL NEW 120V, 20A DUPLEX RECEPTACLE IN ACCESS CONTROL PANEL AND CONNECT BACK TO EXISTING ELECTRICAL PANEL

4	FRONT ADMINISTRATION AREA TO RECEIVE NEW WALL MOUNTED LOCKDOWN BUTTON WITH COVER IN THIS AREA. COORDINATE WITH OWNER ON FINAL LOCATION OF BUTTON PRIOR TO INSTALLATION. CONTRACTOR TO PROVIDE LABELING OF BUTTON TO INDICATE "LOCKDOWN" ON COVER. BUTTON SHALL BE BLUE IN COLOR.

5	APPROXIMATE ROUTE OF MULTICONDUCTOR ACCESS CONTROL CABLE FROM ACCESS CONTROL DOOR BACK TO HEADEND PANEL LOCATED IN MDF/IDF ROOM. CONTRACTOR SHALL BE RESPONSIBLE FOR ALL NEW RACEWAY OR ACCESS PANELS REQUIRED TO INSTALL ACCESS CONTROL WIRING ABOVE INACCESSIBLE CEILINGS. ALL WIRING SHALL BE PROPERLY SUPPORTED FOR FULL RUN. ANY WIRING PENETRATIONS PASSING THRU RATED WALL SHALL MAINTAIN WALL RATING AFTER WIRING IS INSTALLED.

6	LOCATION OF EXISTING 120V ELECTRICAL PANEL. CONTRACTOR TO ROUTE NEW 120V, 20A BRANCH CIRCUIT FROM NEW ACCESS CONTROL PANEL BACK TO THIS LOCATION. CONTRACTOR SHALL INSTALL NEW 120V, 20A BREAKER IN AVAILABLE SPACE IN THIS PANEL.

7	LOCATION OF EXISTING FLOOR MOUNTED NETWORK RACKS. ALL NEW DATA CABLING SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON

EXISTING PATCH PANEL.

8	LOCATION OF EXISTING INTERCOM WALL MOUNTED PUNCHDOWN BLOCK. ALL NEW SPEAKERS SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON TERMINAL STRIP. CONTRACTOR TO CONFIGURE EXISTING INTERCOM SYSTEM TO ADD ANY NEW EXTERIOR SPEAKER AND ZONES TO EXISTING SYSTEM AS REQUIRED.

REYBURN INTERMEDIATE - MULTI-PURPOSE BUILDING SCALE: 1"=20'-0"

9	CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE,
NON-POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION.

10         THIS AREA HAS AN OPEN CEILING AREA OR INACCESSIBLE CEILING AREA, CONDUIT WILL BE REQUIRED TO ROUTE THRU OPEN AREAS OR ACCESS PANELS NEEDED TO ACCESS ABOVE INACCESSIBLE CEILINGS TO ALLOW CABLING TO BE INSTALLED.

11         CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE, POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION. PROVIDE LOCAL POWER TRANSFORMER AND TERMINATIONS REQUIRED TO POWER SPEAKER

DISTRICT-WIDE ACCESS CONTROL UPGRADES PACKAGE #2

MARK	DATE

03/18/24

ISSUE

ISSUE FOR PROPOSAL

ACCESS CONTROL - REYBURN INT. MULTI-PURPOSE BUILDING PLAN

2-RIS-AC18

Page 18 of 20

01 DOOR: RIS-BMPR-DR03	DOOR HARDWARE SET: #08	02 DOOR: RIS-BMPR-DR04	DOOR HARDWARE SET: #08	03 MULTI-PURPOSE BUILDING IDF / ELECTRICAL ROOM

HW GROUP NO. 08	HW GROUP NO. 08	1

QTY	DESCRIPTION

1	EA	ELECTRIC HINGE 1	EA	PANIC HARDWARE
1	EA	ELEC PANIC HARDWARE 1	EA	RIM CYLINDER
1	EA	FSIC CORE

1	EA	CARD READER

POWER SUPPLY

CATALOG NUMBER

5BB1HW 4.5 X 4.5 CON TW8 LD-PA-AX-99-EO-990
QELX-PA-AX-99-NL-CON 20-057 ICX
23-030

BY WORK OF DIVISION 28 BY WORK OF DIVISION 28
RE-USE BALANCE OF EXISTING HARDWARE

FINISH     MFR

652	IVE 626	VON 626	VON 626	SCH
626	SCH

QTY	DESCRIPTION

1	EA	ELECTRIC HINGE 1	EA	PANIC HARDWARE
1	EA	ELEC PANIC HARDWARE 1	EA	RIM CYLINDER
1	EA	FSIC CORE

1	EA	CARD READER

POWER SUPPLY

CATALOG NUMBER

5BB1HW 4.5 X 4.5 CON TW8 LD-PA-AX-99-EO-990
QELX-PA-AX-99-NL-CON 20-057 ICX
23-030

BY WORK OF DIVISION 28 BY WORK OF DIVISION 28
RE-USE BALANCE OF EXISTING HARDWARE

FINISH     MFR

652	IVE 626	VON 626	VON 626	SCH
626	SCH

DISTRICT-WIDE ACCESS CONTROL UPGRADES PACKAGE #2

MARK	DATE

03/18/24

ISSUE

ISSUE FOR PROPOSAL

ACCESS CONTROL - REYBURN INT. PHOTOS - MULTI-PURPOSE BLDG

2-RIS-AC20

Page 20 of 20

1	RE:2-TKE-AC9 TKE-BMPR-DR01

CR

REX

5

10

ACCESS CONTROL - GENERAL NOTES:

ALL LOW VOLTAGE CABLING IN EXPOSED AREAS SHALL BE INSTALLED IN SURFACE MOUNTED RACEWAY OR CONDUIT

ALL EXPOSED CONDUIT IN PUBLIC SPACES SHALL BE PAINTED TO MATCH EXISTING WALL OR CEILING COLOR

ALL ACCESS CONTROL WIRING SHALL BE GREEN IN COLOR

ALL LOW VOLTAGE WIRING NOT INSTALLED IN CONDUIT SHALL BE SUPPORTED EVERY 5' MINIMUM FROM APPROVED CABLING SUPPORT SYSTEM CONNECTED BACK TO BUILDING STRUCTURE

COORDINATE WITH OWNER TECHNOLOGY DEPARTMENT ON LABELING AND TERMINATION PUNCHDOWN OF NEW DATA CABLING ASSOCIATED WITH ACCESS CONTROL SYSTEM

CONTRACTOR TO REPAIR ANY HOLES IN EXISTING DOORS AND FRAMES AS A RESULT OF HARDWARE REPLACEMENT. CONTRACTOR TO REPAINT FRAMES AND DOORS TO MATCH EXISTING SURROUNDING COLOR FOR ANY AREAS EXPOSED WHERE OLD HARDWARE WAS REMOVED.

CONTRACTOR TO COORDINATE WITH OWNER ON ALL PROGRAMMING AND DOOR NUMBERING REQUIREMENTS ASSOCIATED WITH ACCESS CONTROL SYSTEM PRIOR TO ANY WORK TAKING PLACE

CONTRACTOR IS RESPONSIBLE FOR PROVIDING BUILDING MAPS FOR EACH CAMPUS BUILDING AND INTEGRATING WITH ACCESS CONTROL DOOR LOCATIONS TO INDICATE DOOR STATUS AND PROVIDE REMOTE OPERATION OF DOORS THRU ACCESS CONTROL SYSTEM

CONTRACTOR IS REQUIRED TO PROVIDE ALL DOOR HARDWARE, WIRING AND POWER SUPPLIES ASSOCIATED WITH THE INSTALLATION OF ACCESS CONTROL SYSTEM.

CONTRACTOR TO PROVIDE 120V. POWER, CONDUIT, WIRING AND BREAKERS ASSOCIATED WITH PROVIDING POWER TO ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES

CONTRACTOR SHALL COORDINATE WITH OWNER ON THE TRANSITION AND SCHEDULING OF ACCESS CONTROL SYSTEM ONCE ITS READY TO ACTIVATE FOR EACH BUILDING

CONTRACTOR SHALL MAINTAIN EXISTING WALL RATINGS FOR ANY PENETRATIONS THRU EXISTING RATED WALLS AS A RESULT OF ANY NEW CABLING BEING INSTALLED.

CONTRACTOR SHALL INSTALL A REQUEST TO EXIT "REX" DEVICE FOR ALL DOORS RECEIVING A CARD READER AND ELECTRIFIED HARDWARE INTERFACE. REX DEVICE SHALL PROVIDE STATUS OF BOTH DOORS. DEVICE TO BE WALL OR CEILING MOUNTED TO PROVIDE PROPER COVERAGE OF EXIT PATHWAY

ACCESS CONTROL - KEYED NOTES:

1

2

3

CR

REX	1	RE:2-TKE-AC9
TKE-BMPR-DR02	4

THIS DOOR SHALL RECEIVE A NEW CARD READER. CONTRACTOR SHALL REFER TO DOOR HARDWARE SCHEDULE FOR WORK SCOPE REQUIRED. PROVIDE ALL NEW HARDWARE, WIRING AND TERMINATIONS REQUIRED TO INSTALL NEW CARD READER AND ELECTRIFIED DOOR HARDWARE

LOCATION OF EXISTING MDF/IDF ROOM. ALL NEW ACCESS CONTROL PANELS AND DOOR POWER SUPPLIES SHALL BE INSTALLED IN THIS ROOM.

LOCATION OF NEW ACCESS CONTROL PANEL AND DOOR POWER SUPPLIES SHALL BE MOUNTED ON THE WALL AT THIS LOCATION. CONTRACTOR TO INSTALL NEW CATEGORY 6 DATA CABLE FROM NEW ACCESS CONTROL PANEL BACK TO EXISTING PATCH PANEL IN EXISTING DATA RACK AND TERMINATE ON AVAILABLE PORT. CONTRACTOR TO INSTALL NEW WIRING IN SURFACE MOUNTED RACEWAY OR ROUTED ON EXISTING LADDER RACK FROM ACCESS CONTROL PANEL BACK TO RACK. CONTRACTOR TO INSTALL NEW 120V, 20A DUPLEX RECEPTACLE IN ACCESS CONTROL PANEL AND CONNECT BACK TO EXISTING ELECTRICAL PANEL

FRONT ADMINISTRATION AREA TO RECEIVE NEW WALL MOUNTED LOCKDOWN BUTTON WITH COVER IN THIS AREA. COORDINATE WITH OWNER ON FINAL LOCATION OF BUTTON PRIOR TO INSTALLATION. CONTRACTOR TO PROVIDE LABELING OF BUTTON TO INDICATE "LOCKDOWN" ON COVER. BUTTON SHALL BE BLUE IN COLOR.

6		5	5 10
8

1	6

7

7	8

9

1

APPROXIMATE ROUTE OF MULTICONDUCTOR ACCESS CONTROL CABLE FROM ACCESS CONTROL DOOR BACK TO HEADEND PANEL LOCATED IN MDF/IDF ROOM. CONTRACTOR SHALL BE RESPONSIBLE FOR ALL NEW RACEWAY OR ACCESS PANELS REQUIRED TO INSTALL ACCESS CONTROL WIRING ABOVE INACCESSIBLE CEILINGS. ALL WIRING SHALL BE PROPERLY SUPPORTED FOR FULL RUN. ANY WIRING PENETRATIONS PASSING THRU RATED WALL SHALL MAINTAIN WALL RATING AFTER WIRING IS INSTALLED.

LOCATION OF EXISTING 120V ELECTRICAL PANEL. CONTRACTOR TO ROUTE NEW 120V, 20A BRANCH CIRCUIT FROM NEW ACCESS CONTROL PANEL BACK TO THIS LOCATION. CONTRACTOR SHALL INSTALL NEW 120V, 20A BREAKER IN AVAILABLE SPACE IN THIS PANEL.

LOCATION OF EXISTING FLOOR MOUNTED NETWORK RACKS. ALL NEW DATA CABLING SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON EXISTING PATCH PANEL.

LOCATION OF EXISTING INTERCOM WALL MOUNTED PUNCHDOWN BLOCK. ALL NEW SPEAKERS SHALL BE ROUTED BACK TO THIS LOCATION AND TERMINATED ON TERMINAL STRIP. CONTRACTOR TO CONFIGURE EXISTING INTERCOM SYSTEM TO ADD ANY NEW EXTERIOR SPEAKER AND ZONES TO EXISTING SYSTEM AS REQUIRED.

CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE,
NON-POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION.

ADMINISTRATION BLDG - TEMPERANCE-KUTNER ELEMENTARY SCALE: 1/16"=1'-0"

10         THIS AREA HAS AN OPEN CEILING AREA OR INACCESSIBLE CEILING AREA, CONDUIT WILL BE REQUIRED TO ROUTE THRU OPEN AREAS OR ACCESS PANELS NEEDED TO ACCESS ABOVE INACCESSIBLE CEILINGS TO ALLOW CABLING TO BE INSTALLED.

11         CONTRACTOR TO INSTALL NEW WALL MOUNTED, EXTERIOR GRADE, POWERED SPEAKER, WHITE IN COLOR AT THIS LOCATION AND CONNECT BACK TO EXISTING LOCAL BUILDING INTERCOM TERMINAL STRIP AT EXISTING MDF/IDF LOCATION. PROVIDE LOCAL POWER TRANSFORMER AND TERMINATIONS REQUIRED TO POWER SPEAKER

DISTRICT-WIDE ACCESS CONTROL UPGRADES PACKAGE #2

MARK	DATE

03/18/24

ISSUE

ISSUE FOR PROPOSAL

ACCESS CONTROL - TEMPERANCE-KUTNER ES - MPR BUILDING PLAN

2-TKE-AC8

Page 8 of 10